* **Addressing Table**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Device** | **Interface** | **IP Address / Prefix** | | **Default Gateway** |
| R1 | G0/0 | 2001:db8:1:1::1/64 | | N/A |
| *R1* | G0/1 | 10.10.1.97 | 255.255.255.224 | N/A |
| *R1* | S0/0/1 | 10.10.1.6 | 255.255.255.252 | N/A |
| *R1* | *S0/0/1* | 2001:db8:1:2::2/64 | | *N/A* |
| *R1* | *S0/0/1* | fe80::1 | | *N/A* |
| R2 | S0/0/0 | 10.10.1.5 | 255.255.255.252 | N/A |
| *R2* | *S0/0/0* | 2001:db8:1:2::1/64 | | *N/A* |
| *R2* | S0/0/1 | 10.10.1.9 | 255.255.255.252 | N/A |
| *R2* | *S0/0/1* | 2001:db8:1:3::1/64 | | *N/A* |
| *R2* | *S0/0/1* | fe80::2 | | *N/A* |
| R3 | G0/0 | 2001:db8:1:4::1/64 | | N/A |
| *R3* | G0/1 | 10.10.1.17 | 255.255.255.240 | N/A |
| *R3* | S0/0/1 | 10.10.1.10 | 255.255.255.252 | N/A |
| *R3* | *S0/0/1* | 2001:db8:1:3::2/64 | | *N/A* |
| *R3* | *S0/0/1* | fe80::3 | | *N/A* |
| PC1 | NIC | 10.10.1.98 | 255.255.255.224 | 10.10.1.97 |
| PC2 | NIC | 2001:DB8:1:1::2 | | FE80::1 |
| PC3 | NIC | 10.10.1.18 | 255.255.255.240 | 10.10.1.17 |
| PC4 | NIC | 2001:DB8:1:4::2 | | FE80::2 |

* **Objectives**

**Part 1: Test and Restore IPv4 Connectivity**

**Part 2: Test and Restore IPv6 Connectivity**

* **Scenario**

There are connectivity issues in this activity. In addition to gathering and documenting information about the network, you will locate the problems and implement acceptable solutions to restore connectivity.

**Note:** The user EXEC password is **cisco**. The privileged EXEC password is **class**.

* **Instructions**
* **Test and Restore IPv4 Connectivity**
* **Use ipconfig and ping to verify connectivity.**
* Click **PC1** and open the **Command Prompt**.
* Enter the **ipconfig /all** command to collect the IPv4 information. Complete the **Addressing Table** with the IPv4 address, subnet mask, and default gateway.
* Click **PC3** and open the **Command Prompt**.
* Enter the **ipconfig /all** command to collect the IPv4 information. Complete the **Addressing Table** with the IPv4 address, subnet mask, and default gateway.
* Use the **ping** command to test connectivity between **PC1** and **PC3**. The ping should fail.
* **Locate the source of connectivity failure.**
* From **PC1**, enter the necessary command to trace the route to **PC3**.

Question:

What is the last successful IPv4 address that was reached?

**A) 10.10.1.97**

***Type your answers here.***

* The trace will eventually end after 30 attempts. Enter **Ctrl**+**C** to stop the trace before 30 attempts.
* From **PC3**, enter the necessary command to trace the route to **PC1**.

Question:

What is the last successful IPv4 address that was reached?

***A) 10.10.1.17***

* Enter **Ctrl**+**C** to stop the trace.

*Open configuration window*

* Click **R1**. Press **ENTER** and log in to the router.
* Enter the **show ip interface brief** command to list the interfaces and their status. There are two IPv4 addresses on the router. One should have been recorded in Step 2a.

Question:

What is the other?

***A) 10.10.1.6***

* Enter the **show ip route** command to list the networks to which the router is connected. Note that there are two networks connected to the **Serial0/0/1** interface.

Question:

What are they?

Type your answers here.

**A) 10.10.1.4/30, 10.10.1.6/32**

* Repeat steps 2e through 2g with **R3** and record your answers.

A) 10.10.1.8/30, 10.10.1.10/32

***Type your answers here.***

* Click **R2**. Press **ENTER** and log into the router.
* Enter the **show ip interface brief** command and record your addresses.

***A) 10.10.1.8/30, 10.10.1.9/32***

* Run more tests if it helps visualize the problem. Simulation mode is available.

*Close configuration window*

* **Propose a solution to solve the problem.**

Compare your answers in Step 2 to the documentation you have available for the network.

Question:

What is the error?

***In R2 s0/0/0 port was inccorectly configured. It was 10.10.1.2 we changed it to 10.10.1.5e your answers here.***

What solution would you propose to correct the problem?

**We went to R2 and wrote the following commands, config terminal > int s0/0/0 > ip address 10.10.1.5 255.255.255.252 to solve the router config problem.**

* **Implement the plan.**

Implement the solution you proposed in Step 3b.

* **Verify that connectivity is restored.**
* From **PC1** test connectivity to **PC3**.
* From **PC3** test connectivity to **PC1**.

Question:

Is the problem resolved?

***A) YES***

* **Document the solution.**
* **Test and Restore IPv6 Connectivity**
* **Use ipv6config and ping to verify connectivity.**
* Click **PC2** and open the **Command Prompt**.
* Enter the **ipv6config /all** command to collect the IPv6 information. Complete the **Addressing Table** with the IPv6 address, subnet prefix, and default gateway.
* Click **PC4** and open the **Command Prompt**.
* Enter the **ipv6config /all** command to collect the IPv6 information. Complete the **Addressing Table** with the IPv6 address, subnet prefix, and default gateway.
* Test connectivity between **PC2** and **PC4**. The ping should fail.
* **Locate the source of connectivity failure.**
* From **PC2**, enter the necessary command to trace the route to **PC4**.

Question:

What is the last successful IPv6 address that was reached?

***TA)2001:DB8:1:3::2ype your answers here.***

* The trace will eventually end after 30 attempts. Enter **Ctrl**+**C** to stop the trace before 30 attempts.
* From **PC4**, enter the necessary command to trace the route to **PC2**.

Question:

What is the last successful IPv6 address that was reached?

***A) NO ipv6 addresses were reached***

* Enter **Ctrl**+**C** to stop the trace.
* Click **R3**. Press **ENTER** and log in to the router.
* Enter the **show ipv6 interface brief** command to list the interfaces and their status. There are two IPv6 addresses on the router. One should match the gateway address recorded in Step 1d.

Question:

Is there a discrepancy?

A) yes

* Run more tests if it helps visualize the problem. Simulation mode is available.
* **Propose a solution to solve the problem.**

Compare your answers in Step 2 to the documentation you have available for the network.

Question:

What is the error?

***A) pc4's default gateway was incorrectly cofigured. we changed it fro FE80::2 to FE80::3***

What solution would you propose to correct the problem?

* **Implement the plan.**

**A) we went to pc4's ip cofing and changed the deafult gateway.**

Implement the solution you proposed in Step 3b.

* **Verify that connectivity is restored.**
* From **PC2** test connectivity to **PC4**.
* From **PC4** test connectivity to **PC2**.

Question:

Is the problem resolved?

***A) YES***

* **Document the solution.**

*End of document*